**VESSEL PARTICULARS**

**M/V TSS PEARL**

|  |  |
| --- | --- |
| **CALL SIGN : 3FSL5** | **IMO NO. : 9339868** |
| **OFFICIAL NO. : 111638** | **MMSI : 373599000** |
| **INM** |  |
|  |  |
| **E-MAIL :** **tsspearl@gtmailplus.com** |  |

**VESSEL INFORMATION**

|  |  |
| --- | --- |
| **REGISTERED OWNER: TEHAMA SHIPPING** |  |
| **TYPE OF VESSEL: FULL CONTAINER CARRIER** | **PREVIOUS NAME: ESPERANZA N** |
|  |  |
| **CLASSIFICATION: 100 A5 NAV-0 BWM SOLAS II-2** | **NATIONALITY/ FLAG : PANAMA** |
| **L O A : 190.94 M** | **PORT OF REGISTRY : PANAMA** |
| **SUMMER DRAFT : 11.50 M** | **BREADTH : 28.50 M** |
| **LIGHT SHIP : 11359 T** | **SUMMER DWT : 27155 T** |
| **GROSS TONNAGE : 23633 T** | **NET TONNAGE : 10899 T** |
| **SUEZ GT :70131.44** | **SUEZ NT : 58162.03** |
| **HEIGHT KEEL TO TOP MAST :54.40 M** | **DEPTH MOULDED : 16.80 M** |
|  |  |

**BUILDING INFORMATION**

|  |  |
| --- | --- |
| **BUILDER ZHEJIANG SHIPYARD - NINGBO** | **DELIVERY DATE : 03-FEB-2008** |
| **CLASS DNV GERMANISCHER LIoyd (GL)** | **CLASS REG. NO. : 111638** |
| **MAIN ENGINE MAN B & W**  **8S 60 ME - C** | **SERVICE & MAX SPD. : 18.5 KTS & 21.0 KTS** |
| **M.E POWER : 19040 KW** |
| **TYPE OF PROPELLER : FIXED 5 BLADES** | **BOW THRUSTER : 1442.2 BHP** |
| **VESSEL OF OPERATING UMS YES** |  |

**CAPACITIES**

|  |  |
| --- | --- |
| **CONTAINERS 2011 TEU** | **CARGO HOLDS 888 TEU** |
| **BALLAST 9873.00 CBM** | **ON DECK 1123** |
| **FUEL OIL – HFO 3125.00 CBM** | **DIESEL OIL – MDO 203.90 CBM** |

**MAKERS OF MAIN EQUIPMENT**

|  |  |
| --- | --- |
| **MAIN ENGINE MAN B & W**  **8S 60 ME - C** | **AUXILIARY ENGINES MAK**  **4 X 1530 KW 9M20** |
| **STEERING GEAR ROLLS ROYCE** | **SEPARATORS WESTFALIA** |
| **CARGO CRANES LIEBHERR 3 X 45 T** | **ME AUTOMATION MAN B & W** |
| **RADARS SAM ELECTRONICS** | **GYRO COMPASS ANSCHUTZ** |
| **AUTO PILOT ANSCHUTZ** | **COMMUNICATION DEBEG - SAM** |